REAR WIPER MOTOR REMOVAL/INSTALLATION

id091900801400

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Rear wiper arm and blade (See REAR WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

  (2) Liftgate upper trim (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

  (3) Liftgate side trim (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

  (4) Liftgate lower trim (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9wzw00001596

1 | Rear wiper motor connector
2 | Bolt
3 | Rear wiper motor

4. Install in the reverse order of removal.