No.6 DOOR GLASS REVERSES BEFORE IT FULLY CLOSES [POWER WINDOW SYSTEMS (EXTERIOR OPEN/CLOSE FUNCTION)]

id090361977700

6 | Door glass reverses before it fully closes
POSSIBLE CAUSE | • Malfunction in power window motor • Malfunction in battery • Improper installation of door glass

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | • By operating a power window main switch / power window subswitch, operate the door glass. • Does the door glass mis-reverse? | Yes | Inspect the power window motor and repair or replace it. (See POWER WINDOW MOTOR INSPECTION.)
No | Inspect the following parts and repair or replace them. • Power window motor (See POWER WINDOW MOTOR INSPECTION.) • Battery (brownout) • Door glass (improper installation) Note • Depending on the temperature, battery, and voltage condition, the door glass may mis-reverse.