HEADLIGHT CLEANER SYSTEM OPERATION

id091900102200

Auto Operation

• If the washer switch is turned on when the ignition and headlight switches are at the ON position, the headlight cleaner motor operates.
• The headlight cleaner operates only one time for every five times the washer switch is operated.
• If manual operation occurs within two to five times of the washer switch being operated, the number count is reset. Also, if the headlight switch is turned to the OFF and then to the ON position, the count is reset when the washer switch is turned on.

Manual Operation

• If the washer switch is turned on two consecutive times when the ignition and headlight switches are at the ON position, the headlight cleaner motor operates.

ac9wzn00000490

ac9wzn00000488