ON-BOARD DIAGNOSTIC SYSTEM SIMULATION FUNCTION [AY6A-EL, AY6AX-EL]

id0502k1280700

Special Features

• The on-board diagnostic function can drive output parts based on use of the Mazda Modular Diagnostic System (M-MDS).

Simulation Item List

Item | Related to | Unit/Condition | Test condition
--- | --- | --- | ---
LPS | Pressure control solenoid | A | Ignition ON or idling (P or N position)
SSA | Shift solenoid A | On/Off | Ignition ON or idling (P or N position)
SSB | Shift solenoid B | On/Off | Ignition ON or idling (P or N position)
SSC | Shift solenoid C | A | Ignition ON or idling (P or N position)
SSD | Shift solenoid D | A | Ignition ON or idling (P or N position)
SSE | Shift solenoid E | A | Ignition ON or idling (P or N position)
SSF | Shift solenoid F | A | Ignition ON or idling (P or N position)
TCCC | TCC control solenoid | A | Ignition ON or idling (P or N position)