Bluetooth UNIT REMOVAL/INSTALLATION

id092000833300

L.H.D.

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Disconnect the connector.

ac9uuw00004610

4. While pressing the tabs of the clip A in the direction of arrows (1) shown in the figure, press the clip A in the direction of arrow (2) to detach it from the Bluetooth unit.

ac9wzw00002936

5. Remove the clip A.

6. While pressing the tabs of the clip B in the direction of arrows (1) shown in the figure, press the clip B in the direction of arrow (2) to detach it from the Bluetooth unit.

7. Remove the clip B.

8. Remove the nuts.

ac9uuw00004612

9. Remove in the Bluetooth unit.

10. Remove the screws.

ac9wzw00003034

11. Remove the washers.

12. Remove the Bluetooth unit from the bracket.

13. Install in the reverse order of removal.

R.H.D.

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Passenger side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

ac9wzw00001131

1 | Connector
2 | Screw
3 | Nut
4 | Bluetooth unit

5. Remove the screws.

ac9wzw00003035

6. Remove the washers.

7. Remove the Bluetooth unit from the bracket.

8. Install in the reverse order of removal.