CYLINDER BLOCK CONSTRUCTION [MZI-3.7]

id0110c5100500

• Aluminum alloy has been adopted on the cylinder block, which consists of a cylinder block and a main bearing cap support.
• The cylinders are numbered 1, 2, 3 from the front along the right bank and 4, 5, 6 from the front along the left bank.
• The liner is cast into each cylinder.
• The main bearing cap support has been adopted to increase the rigidity.

ac9wzn00000673