VANITY MIRROR ILLUMINATION BULB REMOVAL/INSTALLATION

id091800808200

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

ampjjw00002955

1 | Lens (See Lens Removal Note.)
2 | Vanity mirror illumination bulb

3. Install in the reverse order of removal.

Lens Removal Note

1. Insert a tape-wrapped flathead screwdriver into the service hole, and pry it in the direction indicated by the arrow to remove the lens.

ac9uuw00004682