DTC B1342 [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id09021g802100

DTC B1342 | Keyless control module internal malfunction
--- | ---
DETECTION CONDITION | Malfunction in the keyless control module internal circuit
POSSIBLE CAUSE | Keyless control module malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT KEYLESS CONTROL MODULE • Clear the DTC using the M-MDS. • Turn the ignition switch to the ON position. • Is the DTC displayed? ― M-MDS: B1342 | Yes | Replace the keyless control module and perform the resetting procedure for the advanced keyless system when replacing the keyless control module. (See KEYLESS CONTROL MODULE REMOVAL/INSTALLATION [ADVANCED KEYLESS ENTRY AND START SYSTEM].)
No | DTC troubleshooting completed.