AUTOMATIC TRANSAXLE FEATURES [AY6A-EL, AY6AX-EL]

id0517k3222500

Torque Converter Clutch (TCC) Control and Slip Control

• Based on output speed signals, signals from the PCM (engine speed and accelerator pedal depressing amount) and vehicle speed, smooth TCC control is performed. Also, the slip rate is detected by adding input speed signals, and slip control is performed.

Self Learning Control

• Since TCM performs shift control learning and garage shift control learning, it provides smooth clutch engagement at gear shifting and smooth and delicate shifting while driving.

Manual Mode Shift Control

• By moving the selector lever from the “D position” into the manual shift position and shifting into + (up-shift) or – (down-shift), the driver can select the desired gear, enabling sporty driving that feels like a manual transaxle.