ON-BOARD DIAGNOSIS SYSTEM OUTLINE [POSITION MEMORY CONTROL SYSTEM]

id091300956400

• Self-diagnosis functions include the failure detection that comprehensively detects the failure of position memory control system-related parts, and memory function that memorizes the detected failure, and the data monitor function that retrieves a particular input and output signal.
• You can retrieve and delete service codes and monitor data by using Mazda Modular Diagnostic System (M-MDS).