METER HOOD REMOVAL/INSTALLATION

id091700800900

1. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (6) Upper column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

2. Detach clips A and pins B by pulling them in the direction of the arrow.

ac9uuw00000281

3. Remove the meter hood.

4. Install in the reverse order of removal.