INTRUDER SENSOR FUNCTION

id091400115300

• The intruder sensor is located in center part of the roof the forward part of the roof.
• The intruder sensor detects movement in the vehicle by ultrasonic waves and sends the detection signal to the theft-deterrent control module.
• An intruder sensor cancel button has been installed on the advanced key. If the intruder sensor cancel button is on while the theft-deterrent system is pre-armed, intruder sensor ultrasonic wave output is cut, and movement detection is stopped.

ac9wzn00000586