FRONT CLIMATE CONTROL UNIT REMOVAL/INSTALLATION

id074000805200

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

3. Remove the screws.

ac9wzw00000925

4. Remove the front climate control unit.

5. Install in the reverse order of removal.