RELAY INSPECTION

id092100800300

Relay type

Terminal type | Part name
4 terminals | Type A | • ACC relay • A/C relay • Back-up light relay • TNS relay • Horn relay • Starter relay • Rear window defroster relay • Headlight relay (HI) • Headlight relay (LO) • Headlight relay (LH) • Headlight relay (RH) • Front fog light relay • Rear fog light relay
Type B | • Front blower relay • Rear blower relay • Cooling fan relay No.1 • Cooling fan relay No.2
Type C | • Fuel pump relay • Main relay No.1 • Main relay No.2

Type A

1. Verify the continuity between the relay terminals.

ac9wzw00001057

  • If not as indicated in the table, replace the relay.

ac9wzw00001058

Type B

1. Verify the continuity between the relay terminals.

ac9wzw00001059

  • If not as indicated in the table, replace the relay.

ac9wzw00001060

Type C

1. Verify the continuity between the relay terminals.

ac9wzw00001061

  • If not as indicated in the table, replace the relay.

ac9wzw00001062