WHEEL APRON PANEL (FRONT) INSTALLATION [PANEL REPLACEMENT]

id098008741200

1. When installing new parts, measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for the plug welding before installing the new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.

4. Weld the 20 locations indicated by (A) and install the engine mount bracket.

5. Install the wheel apron panel (front).

ac9uub00000086