SUSPENSION FEATURES

id020000100200

Improved rigidity and handling stability | • Strut type front suspension and E-type multi-link rear suspension adopted
Improved handling and riding comfort | • Six-point rubber mount system front crossmember adopted • Front shock absorber with large bore piston adopted • Front spring layout optimized • Separated input type front shock absorber mount adopted • Ball-type strut bearings adopted on the front strut upper mount
Enlarged trunk compartment | • Separated positioning of rear shock absorber and coil spring adopted
Improved marketability | • Adhesive-type balance weights adopted
Environmental consideration | • Steel balance weights adopted to reduce the use of lead
Tire condition maintenance assistance | • Tire pressure monitoring system (TPMS) adopted