STEERING SPECIFICATIONS

id060000100300

Item | Specifications
--- | ---
Steering wheel | Outer diameter | (mm {in}) | 372 {14.8}
Lock-to-lock | (turns) | 3.1
Steering gear and linkage | Type | Rack-and-pinion
Rack stroke | (mm {in}) | 164.2 {6.465}
Steering column and shaft | Shaft type | Collapsible
Joint type | 2-cross joint
Amount of tilt | (mm {in}) | 45 {1.8}
Amount of telescope | (mm {in}) | 50 {2.0}
Power steering system | Power assist type | Engine speed sensing
Power steering fluid | Type | ATF M-III, M-V or equivalent (e.g. Dexron®II)
Fluid capacity* (approximate quantity) (L {US qt, Imp qt}) | 1.27 {1.34, 1.11}

* :When reservoir tank is at maximum volume