CONTROL SYSTEM OUTLINE

id074000100100

Improved comfort | • A DUAL switch has been adopted with which different temperature settings are possible for the driver and passenger sides • A rear fully-automatic air conditioner for rear seat passengers has been adopted in the console • A rear control switch has been adopted which enables rear A/C operation and the verification of operation conditions using the rear climate control unit.
Reduced fuel consumption when the A/C is operating | • Refrigerant pressure sensor adopted