FRONT CONSOLE BOX REMOVAL/INSTALLATION

id091700803900

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

3. Remove the screw.

ac9uuw00000405

4. Detach clip A and hooks by pulling them in the direction of the arrow.

5. Disconnect the connector.

6. Remove the front console box.

7. Install in the reverse order of removal.