ENGINE MOUNT DISASSEMBLY/ASSEMBLY [MZI-3.7]

id0110c5806900

No.3 Engine Mount Disassembly/Assembly

  Caution
  • For the No.3 engine mount rubber assembly, perform the bolt tightening work while verifying that the stopper is not pinched between the tightened surfaces.

1. Secure the No.3 engine mount bracket in a vise.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

ac9wzw00002916

1 | Bolt
2 | No.3 engine mount rubber
3 | Stopper
4 | No.3 engine mount bracket

No.1 Engine Mount Disassembly/Assembly

1. Secure the No.1 engine mount rubber in a vise.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

ac9wzw00002051

1 | Insulator
2 | Nut
3 | Dynamic damper
4 | No.1 engine mount bracket
5 | Bolt
6 | No.1 engine mount bracket
7 | No.1 engine mount rubber