BLIND SPOT MONITORING (BSM) OFF SWITCH CONSTRUCTION/OPERATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0922009981e1

Construction

• The BSM OFF switch is built into the cluster switch.
• A push-return (moment) type switch has been adopted.

ac9wzn00000931

Operation

1. When the BSM OFF switch operates, the switch operation signal is sent to the BSM control module.
2. The BSM control module switches the BSM system on/off when it receives the BSM OFF switch operation signal from the BSM OFF switch.

ac9uun00000889