FRONT PLANETARY GEAR COMPONENT AND INPUT SHAFT DISASSEMBLY/ASSEMBLY [AY6A-EL, AY6AX-EL]

id0517k3333000

  Note
  • The following procedure is for replacement of the seal rings only. Replace the transaxle if other repairs are necessary.

1. Disassemble in the order indicated in the figure.

2. Assemble in the reverse order of disassembly.

ac9wzw00002027

1 | Front planetary gear component (See Front Planetary Gear Component Disassembly Note.) (See Front Planetary Gear Component Assembly Note.)
2 | Thrust washer (See Thrust Washer Disassembly Note.) (See Thrust Washer Assembly Note.)
3 | Front planetary sun gear (See Front Planetary Sun Gear, Thrust Bearing And Bearing Race Disassembly Note.) (See Bearing Race, Thrust Bearing And The Front Planetary Sun Gear Assembly Note.)
4 | Thrust bearing (See Front Planetary Sun Gear, Thrust Bearing And Bearing Race Disassembly Note.) (See Bearing Race, Thrust Bearing And The Front Planetary Sun Gear Assembly Note.)
5 | Bearing race (See Front Planetary Sun Gear, Thrust Bearing And Bearing Race Disassembly Note.) (See Bearing Race, Thrust Bearing And The Front Planetary Sun Gear Assembly Note.)
6 | Seal ring (See Seal Ring Disassembly Note.) (See Seal Ring Assembly Note.)
7 | Input shaft

Front Planetary Gear Component Disassembly Note

1. Remove the front planetary gear component from the input shaft.

am6xuw00004231

Thrust Washer Disassembly Note

Front (torque converter side)

1. Remove the thrust washer from the front planetary gear component.

ac9uuw00004069

Rear

1. Remove the thrust washer from the front planetary gear component.

ac9uuw00004070

  Note
  • In some cases, the thrust washer may be detached with the input shaft attached.

Front Planetary Sun Gear, Thrust Bearing And Bearing Race Disassembly Note

1. Remove the front planetary sun gear, thrust bearing and the bearing race from the input shaft.

ac9uuw00004071

  Note
  • If it is difficult to remove the bearing race, pry it off gently using a flathead screwdriver.

Seal Ring Disassembly Note

Front (torque converter side)

1. Remove the seal rings from the input shaft.

am6xuw00004234

Rear

1. Remove the seal rings from the input shaft.

ac9uuw00004138

Seal Ring Assembly Note

Rear

1. Apply ATF to the new seal rings and sliding surface of the input shaft.

2. Compress the new seal rings as shown in the figure. Then install the seal rings to the input shaft.

ac9uuw00004072

  Caution
  • Do not expand the seal rings too much.
  • Be careful not to shorten the seal rings too much, when installing the seal rings.

  Note
  • Verity that seal rings rotate smoothly after installing them.

Front (torque converter side)

1. Apply ATF to the new seal rings and sliding surface of the input shaft.

2. Compress the new seal rings as shown in the figure. Then install the seal rings to the input shaft.

ac9uuw00004073

  Caution
  • Do not expand the seal rings too much.
  • Be careful not to shorten the seal rings too much, when installing the seal rings.

  Note
  • Verify that seal rings rotate smoothly after installing them.

Bearing Race, Thrust Bearing And The Front Planetary Sun Gear Assembly Note

1. Apply ATF to the bearing race and thrust bearing.

2. Install the bearing race and thrust bearing to the input shaft as shown in the figure.

am6xuw00004239

3. Install the front planetary sun gear to the input shaft.

am6xuw00004240

Thrust Washer Assembly Note

Rear

1. Apply yellow petrolatum grease to the thrust washer.

2. Install the thrust washer to the front planetary gear component.

ac9uuw00004396

  Caution
  • Apply yellow petrolatum grease to the mounting surface of the thrust washer so that it does not drop when the front planetary gear component is installed.
  • Do not apply yellow petrolatum grease to the oil holes of the thrust washer.
  • Do not drop the thrust washer.

Front (torque converter side)

1. Apply yellow petrolatum grease to the thrust washer.

2. Install the thrust washer to the front planetary gear component.

ac9uuw00004397

  Caution
  • Apply yellow petrolatum grease to the mounting surface of the thrust washer so that it does not drop when the front planetary gear component is installed.
  • Do not apply yellow petrolatum grease to the oil holes of the thrust washer.
  • Do not drop the thrust washer.

Front Planetary Gear Component Assembly Note

1. Install the front planetary gear component to the input shaft.

am6xuw00004231