DTC TABLE [POWER LIFTGATE (PLG) SYSTEM]

id0902e9347100

DTC | Description | Page
--- | --- | ---
B1311 | Door lock-link switch circuit (unlock) failure | (See DTC B1311 [POWER LIFTGATE (PLG) SYSTEM].)
B1318 | Power supply voltage decreases | (See DTC B1318 [POWER LIFTGATE (PLG) SYSTEM].)
B1342 | PLG control module internal malfunction | (See DTC B1342 [POWER LIFTGATE (PLG) SYSTEM].)
B241A | PLG touch sensor circuit malfunction | (See DTC B241A [POWER LIFTGATE (PLG) SYSTEM].)
B266A | Rotation sensor circuit malfunction | (See DTC B266A [POWER LIFTGATE (PLG) SYSTEM].)
B266B | Rotation sensor A circuit malfunction | (See DTC B266B [POWER LIFTGATE (PLG) SYSTEM].)
B266C | Rotation sensor B circuit malfunction | (See DTC B266C [POWER LIFTGATE (PLG) SYSTEM].)
B266E | Rotation sensor malfunction | (See DTC B266E [POWER LIFTGATE (PLG) SYSTEM].)
B267A | Half latch switch circuit malfunction | (See DTC B267A [POWER LIFTGATE (PLG) SYSTEM].)
B267B | Full latch switch circuit malfunction | (See DTC B267B [POWER LIFTGATE (PLG) SYSTEM].)
B267C | Return switch circuit malfunction | (See DTC B267C [POWER LIFTGATE (PLG) SYSTEM].)
B2699 | PLG touch sensor (LH) circuit malfunction | (See DTC B2699 [POWER LIFTGATE (PLG) SYSTEM].)
B2700 | PLG touch sensor (RH) circuit malfunction | (See DTC B2700 [POWER LIFTGATE (PLG) SYSTEM].)
B2701 | PLG touch sensor (LH) circuit malfunction | (See DTC B2701 [POWER LIFTGATE (PLG) SYSTEM].)
B2702 | PLG touch sensor (RH) circuit malfunction | (See DTC B2702 [POWER LIFTGATE (PLG) SYSTEM].)
B2821 | Closure motor circuit malfunction | (See DTC B2821 [POWER LIFTGATE (PLG) SYSTEM].)
B2936 | PLG motor circuit malfunction | (See DTC B2936 [POWER LIFTGATE (PLG) SYSTEM].)
B2937 | PLG motor circuit malfunction | (See DTC B2937 [POWER LIFTGATE (PLG) SYSTEM].)
B2939 | Clutch circuit malfunction | (See DTC B2939 [POWER LIFTGATE (PLG) SYSTEM].)
U0073 | Unit communication error | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100 | Communication error to PCM
U0101 | Communication error to TCM
U0140 | Communication error to BCM
U0155 | Communication error to instrument cluster
U0214 | Communication error to keyless control module