IGNITION KEY ILLUMINATION OPERATION

id091800101400

Illumination Condition

• The ignition key illumination glows under all of the following conditions:

  ― Driver-side door is open. (Driver-side door switch is on.)
  ― Ignition switch is in the OFF or ACC position.

Cancel Condition

• The ignition key illumination goes out under any of the following conditions:

  ― 15 s have elapsed since the Driver’s door was closed (After Driver’s door switch is off).
  ― Ignition switch is in the ON position. (Ignition switch ON)
  ― With all the doors closed, a lock signal from the keyless entry is received.
  ― Approx. 30 min have elapsed since the Driver’s door open (Driver’s door switch is on)