LICENSE PLATE LIGHT REMOVAL/INSTALLATION

id091800801100

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Liftgate upper trim (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

  (2) Liftgate side trim (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

  (3) Liftgate lower trim (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00000790

1 | Connector
2 | License plate light
3 | Lens
4 | License plate light bulb

4. Install in the reverse order of removal.