COOLING FAN COMPONENT CONSTRUCTION [MZI-3.7]

id0112d3100500

• The cooling fan component consists of the radiator cowling, cooling fans, cooling fan motors, and fan control modules.
• Electric cooling fans No.1 and No.2, which operate according to the fan control signals sent from the PCM to the fan control modules No.1 and No.2, have been adopted. This reduces engine noise and provides rapid engine warming up.
• The radiator cowling and cooling fans are made of plastic for weight reduction.

ac9wzn00000380

Cooling fan, cooling fan motor specification

Item | Specification
--- | ---
No.1 | No.2
Cooling fan | Number of blades | 5 | 7
Outer diameter | (mm {in}) | 360 {14.2}
Cooling fan motor output | (W) | 240