SYMPTOM TROUBLESHOOTING CHART [POWER LIFTGATE (PLG) SYSTEM]

id0903c9812700

No. | SYMPTOM | DESCRIPTION
--- | --- | ---
1 | Does not latch release with liftgate outer handle switch | • The liftgate is not released latch when using the liftgate outer handle switch.
2 | Does not operate liftgate auto closure | • Liftgate is not pulled in from adjure position when the liftgate is closing.
3 | Does not auto open | • Liftgate does not operate auto open. • PLG buzzer does not sound when the PLG front switch and/or transmitter is operated. • Hazard warning light does not flash when the PLG front switch and/or keyless switch is operated.
4 | Does not auto close | • Liftgate does not operate auto close. • PLG buzzer does not sound when the PLG front switch, PLG rear switch and/or transmitter is operated. • Hazard warning light does not flash when the PLG front switch, PLG rear switch and/or keyless switch is operated.
5 | Liftgate reverses and PLG buzzer sounds 3 times, while auto open/close function | • Liftgate reverses while auto open or close operation without object is pinched, the switches (PLG front switch, PLG rear switch and/or transmitter) are operated and/or liftgate outer handle is operated. • PLG buzzer sounds 3 times when the liftgate reverses.
6 | Liftgate reverses and PLG buzzer sounds 1 time, while auto open/close function | • Liftgate reverses while auto open or close operation without object is pinched, the switches (PLG front switch, PLG rear switch and/or transmitter) are operated and/or liftgate outer handle is operated. • PLG buzzer sounds 1 time when the liftgate reverses.
7 | Liftgate open/close speed is unstable while auto open/close function. | • Liftgate operation speed is not stable (be fast or slow reiterate or suddenly) while open or close operation.