SPLASH SHIELD REMOVAL/INSTALLATION

id091600808400

Splash Shield A

1. Remove the bolts.

amxzzw00000972

2. Remove the fasteners at section A shown in the figure.

3. Remove the splash shield A.

4. Install in the reverse order of removal.

Splash Shield B

1. Remove the front suspension tower bar.

2. Remove the splash shield A.

3. Remove the front shock absorber and coil spring.

4. Remove the fasteners at section A shown in the figure.

5. Remove the splash shield B.

amxzzw00000973

6. Install in the reverse order of removal.