SEAT BELT OUTLINE

id081100100400

Improved safety | • Three-point seat belt with the following functions for seat passengers adopted ― ELR (Emergency Locking Retractor: emergency locking mechanism) ― Pre-tensioner seat belt (See PRE-TENSIONER SEAT BELT CONSTRUCTION/OPERATION.) ― Load limiter, which adjusts restraint force of the seat belt to reduce the possibility of injury to passengers caused by excess seat belt pressure after pre-tensioner operation