FUSE SERVICE WARNINGS

id092100801700

  Warning
  • For vehicles with DSC, if the room fuse is disconnected, the stored initial position of the steering angle sensor will be cleared and the DSC will not operate properly, making the vehicle unsafe to drive. Perform the steering angle sensor initialization procedure after connecting the room fuse. (See STEERING ANGLE SENSOR INITIALIZATION PROCEDURE.)