NO.11 TRACK CHANGE IS INOPERATIVE [CD PLAYER/CHANGER]

id0903e5806900

11 | Track change is inoperative
--- | ---
Possible DTC | 10:Er02, 22:Er02
POSSIBLE CAUSE | • Defective CD (e.g., cracked, badly bent, rough edges, scratch, dirty CD, condensation) • Non-conventional discs (e.g., 8 cm (3 in) CD, 8 cm (3 in) disc adapter, heart-shaped disc, octagonal disc) • Center panel malfunction • Audio unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Replace the CD known to be good. • Does the CD player change the track? | Yes | Explain to the customer that the defective CD or non-conventional disc cannot be used.
No | Go to the next step.
2 | • Inspect the center panel installation. • Does the CD player change the track number on the display when pressing the track up or down button? | Yes | Replace the audio unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION). (See CENTER PANEL UNIT DISASSEMBLY/ASSEMBLY).
No | Go to the “No.1 center panel switch inspection” in this section. Replace the center panel as necessary.