CYLINDER BLOCK DISASSEMBLY (I)

id011000500600

1. Disassemble in the order indicated in the table.

belbze00000043

1 | Oil pan
2 | Oil filter cover (cartridge type)
3 | Oil filter
4 | Oil filter adapter
5 | Oil cooler
6 | Gasket
7 | Knock sensor
8 | Oil separator
9 | Thermostat
10 | Water pump
11 | Oil strainer
12 | Oil pump
13 | Flywheel (MTX), Drive plate (ATX) (See Drive Plate (ATX), Flywheel (MTX) Disassembly Note)
14 | End plate (MTX)
15 | Rear oil seal

Drive Plate (ATX), Flywheel (MTX) Disassembly Note

1. Hold the crankshaft using the SST.

2. Remove the bolts in several passes.

belbze00000044