AUDIO SYSTEM SPECIFICATIONS

id092000100400

Audio Unit

Item | Specification
--- | ---
Without Bose® | With Bose®
Rated voltage | (V) | 12
Frequency band | AM | LW | (kHz) | 153—279
MW | (kHz) | 531—1602 (With RDS (radio data system)) 522—1629 (Without RDS (radio data system))
FM | (MHz) | 87.5—108
Audio amplifier maximum output power | (W) | 25 × 4 | External type audio amplifier Tweeter: 18.5 × 2 Door speaker: 74 × 2 Rear speaker: 37 Center speaker: 18.5
Output impedance | (ohm) | 4 | Door speaker: 1 × 2 Rear speaker: 4 × 2 Center speaker: 4

Speaker

Item | Specification
--- | ---
Without Bose® | With Bose®
Door speaker | Tweeter | Rear speaker (with 6 speaker type) | Door speaker | Rear speaker | Door upper speaker | Center speaker
Maximum input | (W) | 25 | 25 | 25 | 81 | 22.5 | 22.5 | 22.5
Impedance | (ohm) | 4 | 4 | 8 | 1 | 3.6 | 3.6 | 3.6
Size | (mm {in}) | 140×190 {5.5×7.5} | 30 {1.2} | 70 {2.8} | 203 {8} | 80 {3.1} | 80 {3.1} | 80 {3.1}