NO.13 NO KICKDOWN [SJ6A-EL]

id050307801800

13 | No kickdown
DESCRIPTION | • Does not downshift when accelerator pedal is fully depressed within kickdown range.
POSSIBLE CAUSE | • If transmission does not downshift though shifting is normal, the malfunction is in the accelerator pedal position, engine speed, throttle position, engine coolant temperature sensor, engine torque signals or TCM (including sensor GND, sensor wiring harness and connector, CAN communication).