UNDERBODY FRONT STRAIGHT-LINE DIMENSIONS [DIMENSIONS]

id098010748000

• The following figure is a bottom view.

d5u0980b020

d5u0980b021

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Front side frame datum hole | ø7 {0.28}
B | Crossmember No.1 datum hole | ø7 {0.28}
C | Engine mounting bolt | M14 {0.55}
E | Engine mounting bolt | M14 {0.55}
F | Front frame rear datum hole | ø16 {0.63}
G | Front frame rear datum slot | ø16 x 20
{0.63 x 0.79}
H | Front B frame datum hole | ø12 {0.47}