LICENSE PLATE LIGHT REMOVAL/INSTALLATION

id091800465800

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Move the license plate light in the direction of the arrow (1) and detach the tab.

amxzzw00001023

4. Pull area A of the license plate light in the direction of the arrow (2) and remove the license plate light.

5. Disconnect the connector.

amxzzw00001024

6. Remove the socket by rotating it in the direction of the arrow shown in the figure.

7. Remove the license plate light bulb.

amxzzw00002149

8. Install in the reverse order of removal.