UNDERBODY REAR STRAIGHT-LINE DIMENSIONS [DIMENSIONS]

id098010748100

• The following figure is a bottom view.

d5u0980b022

d5u0980b023

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
H | Front B frame datum hole | ø12 {0.47}
I | Front B frame datum slot | ø12 x 18
{0.47 x 0.71}
J | Rear side frame datum hole | ø16 {0.63}
K | Rear crossmember mounting bolt | M14 {0.55}
L | Rear crossmember mounting bolt | M14 {0.55}
N | Rear crossmember mounting bolt | M14 {0.55}
O | Rear side frame datum hole | ø16 x 20
{0.63 x 0.79}