DRIVE INFORMATION SYSTEM OPERATION

id092200111200

Drive Information System Switch

• The drive information system switch comprises a set odometer/tripmeter switch.
• The modes can be charged in a cyclic pattern by pressing a set odometer/tripmeter switch.
• The data displayed at the time can be reset by holding a set odometer/tripmeter switch for 1 s or more. Data are calculated as soon as a set odometer/tripmeter switch.

Drive Information System Display

• The display change mode as shown.

Market | Average fuel economy
--- | ---
Except U.K. specs |
U.K. specs |