TROUBLESHOOTING INDEX [ACTIVE BONNET]

id0803f1000700

• For troubleshooting, follow the troubleshooting procedure after verifying the symptom No. on the symptom troubleshooting chart.

No. | Malfunction symptom
--- | ---
1 | Active bonnet warning light does not illuminate when ignition switch is turned to on position.
2 | Active bonnet warning light illuminates immediately after ignition switch is turned to on position and remains illuminated.