DSC OFF SWITCH INSPECTION

id041500802000

L.H.D.

1. Remove the DSC OFF switch. (See DSC OFF SWITCH REMOVAL/INSTALLATION.)

2. Verify that the continuity is as indicated in the table.

  • If not as indicated in the table, replace the DSC OFF switch. (See DSC OFF SWITCH REMOVAL/INSTALLATION.)

  amxzzw00002234

  amxzzw00002235

R.H.D.

1. Remove the DSC OFF switch. (See DSC OFF SWITCH REMOVAL/INSTALLATION.)

2. Verify that the continuity is as indicated in the table.

  • If not as indicated in the table, replace the DSC OFF switch. (See DSC OFF SWITCH REMOVAL/INSTALLATION.)

  amxzzw00002236

  amxzzw00002237