ELECTRICAL SYSTEM

id000000800400

Connectors

Disconnecting connectors

  • When disconnecting a connector, grasp the connectors, not the wires.

  acxuuw00000454

  • Connectors can be disconnected by pressing or pulling the lock lever as shown.

  acxuuw00000455

Locking connector

  • When locking connectors, listen for a click indicating they are securely locked.

  acxuuw00000456

Inspection

  Caution
  • To prevent damage to the terminal, wrap a thin wire around the tester probe before inserting into terminal.

  • When a tester is used to inspect for continuity or measuring voltage, insert the tester probe from the wiring harness side.

  acxuuw00000457

  • Inspect the terminals of waterproof connectors from the connector side since they cannot be accessed from the wiring harness side.

  acxuuw00000458