NO.1 MELTING OF MAIN OR OTHER FUSES [L8, LF]

id0103a0800700

1 | MELTING OF MAIN OR OTHER FUSES
--- | ---
[TROUBLESHOOTING HINTS] • Inspect condition of fuse.

Damaged fuse | Related wiring harness
--- | ---
MAIN | • FAN fuse*1 • Generator • IG KEY 2 fuse • ROOM fuse • ST fuse
ROOM | • DLC-2 • PCM
FUEL PUMP | • Fuel pump relay ― Fuel pump unit
IG KEY1 | • Ignition switch ― ENGINE fuse • Ignition relay
IG KEY2 | • Ignition switch ― Starter relay
ETV | • Drive-by-wire-relay ― PCM • Main relay ― PCM
EGI COMP1 | • EGR valve • OCV (if equipped) • Purge solenoid valve • Variable intake air solenoid valve • Variable tumble solenoid valve (if equipped)
EGI COMP2 | • Drive-by-wire-relay • MAF sensor • PCM
EGI INJ | • Fuel injector No.1 • Fuel injector No.2 • Fuel injector No.3 • Fuel injector No.4
ENGINE*2 (15 A) | • Fuel pump relay • Condenser • Ignition coil No.1 • Ignition coil No.2 • Ignition coil No.3 • Ignition coil No.4 • A/F sensor • HO2S
ENGINE*2 (7.5 A) | • Ignition relay
FAN*1 (30 A) | • Cooling fan relay No.1 ― Cooling fan motor • Cooling fan relay No.2 ― Cooling fan motor
FAN*1 (7.5 A) | • Cooling fan relay No.1 ― PCM • Cooling fan relay No.2 ― PCM • Cooling fan relay No.3 ― PCM
ST | • Starter relay ― Starter

*1 :Two FAN fuses differs in a current value
*2 :Two ENGINE fuses differs in a current value