AUDIO SYSTEM OUTLINE

id092000111000

• A center panel unit with the audio unit and climate control unit installed, and the following equipment built into the center panel has been adopted.

  ― Center panel switch
  ― Display

• Two types of audio units, TYPE A (AM/FM tuner, MP3/WMA (windows media audio) applicable CD player-integrated) and TYPE B (AM/FM tuner, MP3/WMA (windows media audio) applicable CD changer-integrated), are provided.
• ALC (auto level control) function has been adopted. (Without Bose®)
• The noise-response sound compensation system (AudioPilot®2*) has been adopted. (with Bose®)
• All alphabetic character information related to the audio system is displayed on the display in the center panel.
• Three types of speakers have been provided as follows:

4 speaker type
  ― Door speaker
  ― Tweeter

6 speaker type
  ― Door speaker
  ― Tweeter
  ― Rear speaker

7 speaker type (With Bose®)
  ― Door speaker
  ― Rear speaker
  ― Door upper speaker
  ― Center speaker

• A manual antenna with a removable antenna rod has been adopted.
• A condenser has been installed on the high-mount brake light for improved noise reduction.
• Audio control switches on the left spoke of the steering wheel have been adopted.
• Auxiliary jack adopted which can connect to commercially available portable audio, and output sound from speakers via audio unit.
* :AudioPilot®2 is a registered trademark of Bose® Corporation.