COUPLER COMPONENT OUTLINE [SJ6A-EL]

id051311325900

• The coupler component are installed on the transmission case as the grouped connectors of the TFT sensor and solenoids.

ar8wzn00000079

Terminal No. | Signal
--- | ---
A | TFT sensor (-)
B | TFT sensor (+)
C | Shift solenoid G (-)
D | Shift solenoid G (+)
E | Shift solenoid F (-)
F | Shift solenoid F (+)
G | TCC control solenoid (-)
H | TCC control solenoid (+)
I | Line pressure control solenoid (-)
J | Line pressure control solenoid (+)
K | Shift solenoid E
L | Shift solenoid D
M | Shift solenoid C
N | Shift solenoid B
O | Shift solenoid A