JACKING POSITIONS

id000000801300

  Warning
  • Improperly jacking a vehicle is dangerous. The vehicle can slip off the jack and cause serious injury. Use only the correct front and rear jacking points and block the wheels.

• Use safety stands to support the vehicle after it has been lifted.

  Note
  • To prevent obstruction between the jack body and front bumper when the jack body is inserted, use a low-floor type jack.

Front
• Near the center of the front crossmember.
Rear
• At the center of the rear differential.

amxzzw00001869