DRIVE INFORMATION SYSTEM CONSTRUCTION

id092200111300

Average Fuel Economy Mode

• Average fuel economy is calculated from the trip distance and the fuel consumption from the time when the battery is last connected or the average fuel economy data is reset.
• Average fuel economy is updated every 1 min.
Calculation
• Average fuel economy (L/100 km)= Cumulative fuel consumption (L) / Cumulative trip distance (km) × 100
• Average fuel economy (mile/gallon)= Cumulative trip distance (mile) / Cumulative fuel consumption (gallon)
• When the cumulative trip distance is 0 km (0 mile) (vehicle has not traveled since battery was last connected or average fuel economy function was last reset), <99.9 L/100 km> or <0.0 mpg> is displayed.
• When the set odometer/tripmeter switch is pressed for 1 s or more while displaying the average fuel economy, the cumulative fuel consumption data and cumulative trip distance data are reset.
• After the data are reset, <--- L/100 km> or <--- mpg> is displayed for 1 min.