SHIFT MECHANISM OUTLINE [M15M-D]

id051110104000

Detent Spring

• Due to the addition of anti-friction material between the detent springs and balls, hiss and rasping feeling have been greatly reduced, thus improving shift feeling.

Shift Return Spring

• Due to the use of a low spring constant and high set load type 1-2 return spring, the neutral position is crisply felt when shifting from 1-2 or 5-R, thus improving the secure shift feeling.