KEYLESS ENTRY SYSTEM ON-BOARD DIAGNOSIS [KEYLESS ENTRY SYSTEM]

id0903d2800400

  Note
  • When the trunk lid opener cancel switch is at the ON position, the trunk lid does not unlock even when the trunk lid button is pressed. Verify that the trunk lid cancel switch is at the OFF position when performing the on-board diagnostic test.
  • The trunk lid opener cancel switch is located in the trunk compartment.
  • “All doors” includes the trunk lid.

amxzzw00002147