RELAY INSPECTION

id092100800300

Relay type

Terminal type | Part name
Type A | • Main relay • Starter relay • Drive-by-wire relay • Blower relay • Fuel pump relay • Front fog light relay • A/C relay • TNS relay • Rear window defroster relay • Horn relay • Cooling fan relay No.1 • Cooling fan relay No.2 • Cooling fan relay No.3 • Trunk lid opener relay • Rear fog light relay
Type B | • Headlight relay • Ignition relay

Type A

1. Verify the continuity between the relay terminals.

a6e8110w118

  • If not as indicated in the table, replace the relay.

d5e921zw6004

Type B

1. Verify the continuity between the relay terminals.

a6e8110w125

  • If not as indicated in the table, replace the relay.

chu0921w006