SYMPTOM TROUBLESHOOTING CHART [HEADLIGHT AUTO LEVELING SYSTEM]

id0903d0812700

NO. | SYMPTOM | DESCRIPTION
--- | --- | ---
1 | No.1 AUTO LEVELING WARNING LIGHT ILLUMINATES WHEN THE IGNITION SWITCH TURNED TO ON POSITION [HEADLIGHT AUTO LEVELING SYSTEM] | —
2 | No.2 AUTO LEVELING SYSTEM DOES NOT ADJUST OPTICAL AXIS OF THE HEADLIGHTS FOR VEHICLE POSTURE [HEADLIGHT AUTO LEVELING SYSTEM] | • Auto leveling does not adjust optical axis of the headlights for cargo and passenger weight conditions when the vehicle speed above 30 km/h {19 mph}. • Left or right side auto leveling does not operate.